**Scoring Guide**

**Cabinet**

**Construction**

**Points earned \_\_\_\_\_\_\_\_\_/1000 Name\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Door**

1. Fits squarely with the cabinet 0 10 20 30 40 50
2. Routered edge has no burns or deviations 0 10 20 30 40 50
3. Joints are square and have no gaps 0 10 20 30 40 50
4. Hinges are mounted properly 0 10 20 30 40 50
5. Knob/Handle mounted correctly 0 10 20 30 40 50
6. Rabbett is 3/8” x 3/8” 0 10 20 30 40 50 Total\_\_\_\_\_\_\_/300

**Frame/cabinet**

1. Cabinet is square 0 10 20 30 40 50
2. Stiles and rails are square 0 10 20 30 40 50
3. Base trim has no gaps next to cabinet 0 10 20 30 40 50
4. Grain of bottom is oriented correctly 0 10 20 30 40 50
5. Face frame has no gaps 0 10 20 30 40 50
6. Rabbet on back is cut properly 0 10 20 30 40 50
7. Cabinet is level 0 10 20 30 40 50
8. Holes are drilled properly for shelf 0 10 20 30 40 50
9. Shelf is level 0 10 20 30 40 50

Total\_\_\_\_\_\_\_/450

**Laminate Top**

1. Top is anchored securely to the cabinet 0 10 20 30 40 50

Total \_\_\_\_\_\_\_/50

**Shelf**

1. Has less than ¼” side to side movement 0 10 20 30 40 50
2. Front lip is glued properly 0 10 20 30 40 50

Total\_\_\_\_\_\_\_/100

**Back**

1. Masonite back is flush with the cabinet 0 10 20 30 40 50
2. Masonite has no gaps around its perimeter 0 10 20 30 40 50

Total\_\_\_\_\_\_\_/100

**\*Each occurrence is a 10 point deduction**

**F:cabinet scoring guide construction rev spring 2015**