**Machine Lathe Safe and Unsafe Quiz**

**Points earned \_\_\_\_\_/20 Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Directions:** You are to write the letter **U** in the space to the left of the statement if you believe the statement to be **unsafe**. You are to write the letter **S** if you believe the statement to be **safe**.

1. \_\_\_\_\_ To wear safety glasses the entire time you are using the machine lathe.
2. \_\_\_\_\_ To brush chips away with a brush.
3. \_\_\_\_\_ To wear long sleeves when operating the lathe.
4. \_\_\_\_\_ To touch chips with your bare hands.
5. \_\_\_\_\_ To cut within 1” of the chuck.
6. \_\_\_\_\_ To resharpen the tool bit periodically.
7. \_\_\_\_\_ To wear watches and jewelry when operating the lathe.
8. \_\_\_\_\_ To leave the chuck key in the lathe chuck.
9. \_\_\_\_\_ To observe someone else using the lathe.
10. \_\_\_\_\_ To clean the lathe with a rag while it is running.
11. \_\_\_\_\_ To apply lubricant to the moving parts of lathe.
12. \_\_\_\_\_ To wipe off tapers before putting them into tool holders.
13. \_\_\_\_\_ To tighten the tailstock assembly to the bed of the lathe.
14. \_\_\_\_\_ To wear gloves when working on the machine lathe.
15. \_\_\_\_\_ To take measurements while the lathe is on.
16. \_\_\_\_\_ To turn off the lathe immediately if a strange noise is heard.
17. \_\_\_\_\_ To use the cross feed device to face the end of a work piece
18. \_\_\_\_\_ To use compressed air to clean chips from the lathe.
19. \_\_\_\_\_ To periodically make sure the ball bearing tailstock is against the work surface.
20. \_\_\_\_\_ To always turn the lathe to the “#1” position when turning it on.

F:machine lathe safety quiz