**Scoring Guide**

**Cabinet**

**Finishing**

**Points earned \_\_\_\_\_\_\_\_\_/1000 Name\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Laminate Top**

1. Front laminate is trimmed properly 0 10 20 30 40 50
2. Left side laminate trimmed properly 0 10 20 30 40 50
3. Right side laminate trimmed properly 0 10 20 30 40 50
4. No chips or burns on the plastic laminate 0 10 20 30 40 50
5. No glue is present on the surface 0 10 20 30 40 50
6. Top perimeter edge filed/dressed correctly 0 10 20 30 40 50

Total\_\_\_\_\_\_\_/300

**Door**

1. Door front sanded correctly 0 10 20 30 40 50
2. Door edges sanded correctly 0 10 20 30 40 50
3. No glue on door plywood face 0 10 20 30 40 50

Total \_\_\_\_\_\_\_\_/150

**Blemishes/Filling**

1. Stiles and rails have no gaps or filler 0 10 20 30 40 50
2. Trim joints have no gaps or filler 0 10 20 30 40 50
3. 12. Nails countersunk 0 10 20 30 40 50
4. 13. Countersunk nails filled with wood filler 0 10 20 30 40 50

Total \_\_\_\_\_\_\_\_200

**Surface Finishing**

1. Cabinet is sanded properly 0 10 20 30 40 50
2. No sanding through surface veneers 0 10 20 30 40 50
3. No glue is showing through the stain 0 10 20 30 40 50
4. Stain has no streaking 0 10 20 30 40 50
5. Lacquer has no runs 0 10 20 30 40 50
6. Lacquer has no voids or streaking 0 10 20 30 40 50
7. Lacquer is smooth with no rough areas 0 10 20 30 40 50

Total \_\_\_\_\_\_\_\_/350

F:cabinet scoring guide finishing rev spring 2015