**Router**

**Safe and Unsafe Quiz**

**Points earned \_\_\_\_\_\_\_\_/18 Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Directions:** After viewing a class demonstration you are to respond to the following statements by writing an S for statements that you believe to be safe and a U for statements you believe to be unsafe. When finished turn you paper face down. NO TALKING.

1. \_\_\_\_\_ To wear safety glasses the entire time when using the router.

2. \_\_\_\_\_ To ensure everyone around has on their safety glasses when using the router.

3. \_\_\_\_\_ To make several light cuts instead on one heavy one.

4. \_\_\_\_\_ To allow the motor to stop before setting the router down.

5. \_\_\_\_\_ To place the router upside down on the table when not in use.

6. \_\_\_\_\_ To make sure the cutter is secure before routing.

7. \_\_\_\_\_ To keep the router away from the wood when turning the router on.

8. \_\_\_\_\_ To always assume the router is set to the correct depth.

9. \_\_\_\_\_ To have someone else hold onto the work piece when routing.

10. \_\_\_\_\_ To route from left to right (counter clockwise) when on the edge of a work piece.

11. \_\_\_\_\_ To have the work piece securely clamped with two (2) C-clamps.

12. \_\_\_\_\_ To keep the bit against the work piece after turning the router off.

13. \_\_\_\_\_ To make sure the switch is off prior to plugging the router in.

14. \_\_\_\_\_ To continue to use a router bit that is causing smoke or is burning your wood.

15. \_\_\_\_\_ To keep the router flat and level when routing.

16. \_\_\_\_\_ To make sure all loose clothing is secure prior to routing.

17. \_\_\_\_\_ To test the router bit on scrap before routing your work piece

18. \_\_\_\_\_ To change bits or make adjustments with the router plugged in.

f:routersafetyquiz